**Assignment -4**

| Assignment Date | 30 October 2022 |
| --- | --- |
| Student Name | Kokila N |
| Student Roll Number | 910019106021 |
| Maximum Marks | 2 Marks |

**Question :**

Write a code and connections in wokwi for the ultrasonic sensor. Whenever the distance is less than 100cms send an “Alert” to IBM cloud and display in the device recent events.

# Code:

#include <WiFi.h> #include <PubSubClient.h>

void callback(char\* subscribetopic, byte\* payload, unsigned int payloadLength);

//-------credentials of IBM Accounts------

#define ORG "jqr6mg"//IBM ORGANITION ID

#define DEVICE\_TYPE "generaldevice"//Device type mentioned in ibm watson IOT Platform #define DEVICE\_ID "generaldevice"//Device ID mentioned in ibm watson IOT Platform #define TOKEN "25214317" //Token

String data3;

char server[] = ORG ".messaging.internetofthings.ibmcloud.com"; char publishTopic[] = "iot-2/evt/Data/fmt/json";

char subscribetopic[] = "iot-2/cmd/test/fmt/String"; char authMethod[] = "use-generaldevicetoken-auth";

char token[] = TOKEN;

char clientId[] = "d:" ORG ":" DEVICE\_TYPE ":" DEVICE\_ID;

WiFiClient wifiClient;

PubSubClient client(server, 1883, callback ,wifiClient); const int trigPin = 5;

const int echoPin = 18; #define SOUND\_SPEED 0.034 long duration;

float distance; void setup() {

**Serial**.begin(115200); pinMode(trigPin, OUTPUT); pinMode(echoPin, INPUT); wificonnect(); mqttconnect();

}

void loop()

{

digitalWrite(trigPin, LOW); delayMicroseconds(2); digitalWrite(trigPin, HIGH); delayMicroseconds(10); digitalWrite(trigPin, LOW); duration = pulseIn(echoPin, HIGH); distance = duration \* SOUND\_SPEED/2; **Serial**.print("Distance (cm): "); **Serial**.println(distance); if(distance<100)

{

**Serial**.println("ALERT!!"); delay(1000);

PublishData(distance); delay(1000);

if (!client.loop()) { mqttconnect();

}

}

delay(1000);

}

void PublishData(float dist) { mqttconnect();

String payload = "{\"Distance\":"; payload += dist;

payload += ",\"ALERT!!\":""\"Distance less than 100cms\""; payload += "}";

**Serial**.print("Sending payload: ");

**Serial**.println(payload);

if (client.publish(publishTopic, (char\*) payload.c\_str())) {

**Serial**.println("Publish ok");

} else {

**Serial**.println("Publish failed");

}

}

void mqttconnect() {

if (!client.connected()) { **Serial**.print("Reconnecting client to "); **Serial**.println(server);

while (!!!client.connect(clientId, authMethod, token)) {

**Serial**.print("."); delay(500);

}

initManagedDevice();

**Serial**.println();

}

}

void wificonnect()

{

**Serial**.println(); **Serial**.print("Connecting to "); WiFi.begin("Wokwi-GUEST", "", 6); while (WiFi.status() != WL\_CONNECTED) { delay(500);

**Serial**.print(".");

}

**Serial**.println(""); **Serial**.println("WiFi connected"); **Serial**.println("IP address: "); **Serial**.println(WiFi.localIP());

}

void initManagedDevice() {

if (client.subscribe(subscribetopic)) { **Serial**.println((subscribetopic)); **Serial**.println("subscribe to cmd OK");

} else {

**Serial**.println("subscribe to cmd FAILED");

}

}

void callback(char\* subscribetopic, byte\* payload, unsigned int payloadLength)

{

**Serial**.print("callback invoked for topic: ");

**Serial**.println(subscribetopic);

for (int i = 0; i < payloadLength; i++) {

//Serial.print((char)payload[i]); data3 += (char)payload[i];

}

**Serial**.println("data: "+ data3); data3="";

}

# Diagram.json:

{

  "version": 1,

  "author": "Kokila N",

  "editor": "wokwi",

  "parts": [

    { "type": "wokwi-esp32-devkit-v1", "id": "esp", "top": -31.21, "left": -107.74, "attrs": {} },

    { "type": "wokwi-hc-sr04", "id": "ultrasonic1", "top": -81.19, "left": 86.48, "attrs": {} }

  ],

  "connections": [

    [ "esp:TX0", "$serialMonitor:RX", "", [] ],

    [ "esp:RX0", "$serialMonitor:TX", "", [] ],

    [

      "ultrasonic1:VCC",

      "esp:VIN",

      "red",

      [ "v26.91", "h-139.87", "v-90.66", "h-143.91", "v10.14" ]

    ],

    [ "ultrasonic1:GND", "esp:GND.1", "black", [ "v102.36", "h-186.36" ] ],


    [ "ultrasonic1:TRIG", "esp:D5", "green", [ "v46.57", "h-177.56" ] ],

    [ "ultrasonic1:ECHO", "esp:D18", "green", [ "v38.33", "h-183.55" ] ]


  ]

}

Crcuit Diagram:

**Output:**

Wokwi output:



# IBM cloud output:

